# Brailliant 14 Getting Started

Thank you for purchasing the Brailliant 14 braille display. This display combines a comfortable and simple braille display experience with efficient note taking and synchronization.

Prior to using your Brailliant, ensure it is charged completely. Connect the small end of the included micro USB cable to the port located on the left edge of the Brailliant, just in front of the power button. Plug the larger end of the cable into the included wall charger and plug into the wall. You should see “Charging” on the display. Note you can use other USB wall chargers but charging speeds may be slower.

When charged, you can turn on the Brailliant 14 by holding the power button located on the left edge of the device, just behind the charging port for 3 seconds. Hold the power button again to turn the device off.

On the front edge of the Brailliant you will find HumanWare’s signature thumb keys. The two outer keys are previous and next, navigating you to the previous or next items, and the two inner keys are left and right. These inner keys pan the display left or right. Above each of the 14 braille cells are cursor router touch sensors. Simply slide your finger up from a cell and you will touch the cursor router sensor. You can configure the sensitivity in the settings menu.

Near the braille input keys dot 1 and 4 you will find the Brailliant’s navigation joystick. Pressing in on this joystick selects items.

On the back edge of the device is the mode switch. With the Brailliant in front of you ready for use, sliding that switch to the right puts the Brailliant in braille terminal mode and it is ready to be paired with a smartphone or computer. Sliding the switch to the left puts it in application mode where you can access the Notes and Stopwatch applications.

**To pair your Brailliant 14 with an iPhone running iOS 10.3 or later do the following:**

You pair your Brailliant 14 with your iPhone running iOS 10.3 or later via the standard Voiceover method.

On your Brailliant 14 ensure the toggle switch is to the right and the unit is on. This ensures the Brailliant is in terminal mode and ready to be paired with devices.

From the home screen activate settings. Activate General. Activate accessibility. Activate Voiceover. Activate Braille. If Bluetooth is not turned on you will be prompted to do so now

At the bottom of the list you will now find the Brailliant 14. Activate it and it will immediately pair

**To take notes on your Brailliant:**

Download the Brailliant Sync app from the App store. Ensure your Bluetooth on your iPhone is turned on. On your home screen double tap to activate the Brailliant Sync app. Ensure your Brailliant is paired with your phone and double tap “Select Brailliant Device, if one is not found. Double tap on your Brailliant to ensure you are syncing with the correct device. Now double tap on ad an account. Select if you have a Google or other account by double tapping on the appropriate item. Fill in your account info, double tapping on the save item in the top right corner of the screen when done.

**Slide your switch on the back of the Brailliant to the left to set it in application mode and use your thumb keys or joystick to navigate to the Notes application. Select your email account and press space with N (Dots 1-3-4-5), to create a new note. While in the notes application, the following keyboard shortcuts are available:**

 New line: joystick action, dot8

Backspace: space+dot1+dot2, or dot7

Previous line: space + dot1, joystick up

Next line (paragraph): space + dot4, joystick down

Previous word: space + dot2

Next word: space + dot5

Previous character: space + dot3, joystick left

Next character: space+dot6, joystick right

Jump to beginning of note: space+dot1+dot2+dot3

End of the note: space+dot4+dot5+dot6

Save without exiting: space+ S, dot2+dot3+dot4

Save and exit: space+ E, dot1+dot5

Exit without saving Space + Z, Dots 1-3-5-6

In notes list, delete note Space with D (Dots 1-4-5)

In notes list, force sync Space with S (Dots 2-3-4)

For the complete user guide please see the included CD or visit [www.humanware.com](http://www.humanware.com)